                                                                  June 25, 1998 1-1

               Section

                                1

                                                                           Introduction to the HDF APIs

                                             1.1 Overview of the HDF Interfaces

                                                                  The HDF library structure consists of two interface layers and one application layer built upon a

                                                                  physical file format. (See Figure 1a.) The first layer, or the low-level interface , is generally

                                                                  reserved for software developers because it provides support for low-level details such as file I/O,

                                                                  error handling, and memory management. The second layer, containing the single and multifile

                                                                  application interfaces , consists of a set of interfaces designed to simplify the process of storing

                                                                  and accessing data. The single-file interfaces operate on one file at a time, whereas the multifile

                                                                  interfaces can operate on several files simultaneously. The highest HDF layer includes various

                                                                  NCSA and commercial applications and a collection of command-line utilities that operate on

                                                                  HDF files or the data objects they contain.

FIGURE 1a

                                                                  Three Levels of Interaction  with  the HDF File

                                             1.2 Low-Level Interface

                                                                  This is the layer of HDF reserved for software developers and provides routines for error handling,

                                                                  file I/O , memory management, and physical storage. These routines are prefaced with ´H´. For a

                                                                  more detailed discussion of the low-level interface, consult the HDF Specification and Devel-

                                                                  oper’s Guide .

HDF File

Data Descriptor Block Data Elements

                                                                             File Header

Low-level Interface  (Routines starting with H)

General Applications

Commercial Applications

NCSA Applications
                                                                                                         Utilities

Multifile APIs
General
Raster

Scientific
 Data

Annotations

Vgroups Vdata

                                                                                                                    Single-file APIs
                                                                          Scientific
                                                                               Data

8-Bit
 Raster  Raster

24-Bit
Annotations

                                                                                                       Palette

1-2 June 25, 1998

                                                                  The low-level interface provides a collection of routines that are prefaced with either ´H ´, ´HE´, or

                                                                  ´HX´.  The H routines are for managing HDF files.  The HE routines provide error handlings.  The

                                                                  HX routines are for managing HDF external files.

                                                                  Prior to H DF version 3.2, all low-level routines began with the prefix ´DF´. As of HDF version

                                                                  3.3, the DF interface was no longer recommended for use. It is only supported to maintain back-

                                                                  ward compatibility with programs and files created under earlier versions of the HDF  library.

                                            1.3 Multifile Application Interfaces

                                                                  The HDF multifile interfaces are designed to allow  operations on more than one file and more

                                                                  than one data object at the same time. The multifile interfaces provided are AN, GR, SD, VS,

                                                                  VSQ, VF, V, and VH. The AN interface is the multifile version of the DFAN annotation interface.

                                                                  The GR interface is the multifile version of the 8- and 24-bit raster image interfaces. The SD inter-

                                                                  face is the multifile version of the scientific data set interface. The VS , VS Q, and VF interfaces

                                                                  support the vdata model. The V and VH  interfaces provide support for the vgroup data model.

                                                                  Like the single-file interfaces, the multifile interfaces are built upon the low-level H routines.

                                                                  Unlike single-file operations, operations performed via a multifile interface are not implicitly pre-

                                                                  ceded by Hopen  and followed by Hclose . Instead, each series of operations on a file must be pre-

                                                                  ceded by an explicit call to open and close the file. Once the file is opened, it remains open until an

                                                                  explicit call is made to close it. This process allows operations on more than one file at a time.

                                                                  1.3.1 Scientific Data Sets: SD Interface

                                                                  The scientific data set interface provides a collection of routines for reading and writing arrays of

                                                                  data. Multidimensional arrays accompanied by a record of their dimension and number type are

                                                                  called scientific data sets. U nder the multifile interface, scientific data sets may include predefined

                                                                  or user defined attribute records. Each attribute record is optional and describes a particular facet

                                                                  of the environment from which the scientific data was taken.

                                                                  The names of the routines in the multifile scientific data set interface are prefaced by ´SD´. The

                                                                  equivalent FORTRAN-77 routine names are prefaced by śf ´.

                                                                  1.3.2 Annotations: AN Interface

                                                                  The purpose of the AN multifile annotation interface is to permit concurrent operations on a set of

                                                                  annotations that exist in more than one file. Annotations consist of labels and descriptions.

                                                                  The C routine names of the multifile annotation interface are prefaced by the string ´AN´ and the

                                                                  FORTRAN -77 routine names are prefaced by ´af ´.

                                                                  1.3.3 General Raster Images: GR Interface

                                                                  The routines in the GR interface provide multifile operations on general raster  image data sets.

                                                                  The C routine names in the general raster interface have the prefix ´GR´ and the equivalent FOR-

                                                                  TRAN-77 routine names are prefaced by ´mg´.

                                                                  1.3.4

                                                                                            Scientific Data Sets: netCDF Interface

                                                                  The SD interface is designed to be as compatible as possible w ith netCDF, an interface developed

                                                                  by the Unidata Program Center. Consequently, the SD interface can read files written by the

June 25, 1998 1-3
netCDF interface, and the netCDF  interface (as implemented in HDF ) can read both netCDF files

and HDF files that contain scientific data sets.

Further information regarding the netCDF interface routines and their equivalents in the HDF

interface can be found  in the User’s Guide. Additional information on the netCDF interface can

be found in the netCDF User’s Guide available by anonymous ftp from
unidata.ucar.edu

.

1.3.5 Vdata: The VS Interface

The VS interface provides a collection of routines for reading and writing customized tables. Each

table is comprised of a series of records whose values are stored in fixed length fields. In addition

to its records, a vdata may contain four kinds of identifying information: a name, class, data type

and a number of field names.

Routines in the VS interface are prefaced by ´VS´. The equivalent FO RTRAN-77 routine names

are prefaced by v́sf ´.

1.3.6 Vdata Query: VSQ Interface

The VSQ interface provides a collection of routines for inquiring about existing vdata. These rou-

tines provide information such as the number of records in a vdata, its field names, number types,

and name. All routines in the VSQ interface are prefaced by ´VSQ´. The equivalent FORTRAN-

77 routine names are prefaced by v́sq´.

1.3.7 Vdata Fields: VF Interface

The VF interface provides a collection of routines for inquiring about the fields in an existing

vdata. These routines provide information such as the field name, size, order, and number type.

All routines in the VF  interface are prefaced by ´VF ´. There are no equivalent FORTRAN-77

functions.

1.3.8 Vgroups: V Interface

The vgroup interface provides a collection of routines for grouping and manipulating HDF data

objects in the file. Each vgroup may contain one or more vdatas, vgroups, or other HDF data

objects. In addition to its members, a vgroup may also be given a  name and a class.

Every routine name in the vgroup interface are prefaced by ´V´. The equivalent FORTRAN-77

routine names are prefaced by v́f ´.

1.3.9  Vdata/Vgroups: VH Interface

The high-level VH interface provides a collection of routines for creating simple vdatas and

vgroups with a single function call. A ll routines  in this interface are prefaced by ´VH´. The equiv-

alent F ORTRAN-77 routine names are prefaced by v́h´.

1.3.10  Vgroup Inquiry: VQ Interface

The high-level VQ interface provides one routine that returns tag information from a specified

vgroup, and one routine that returns reference number information from a specified vgroup. All C

1-4 June 25, 1998

                                                                  routine names in this interface are prefaced by ´VQ´. The equivalent Fortran-77 routine names are

                                                                  prefaced by v́q´.

                                            1.4 Single-File Application Interfaces

                                                                  The HDF single-file application interfaces include several independent modules each is designed

                                                                  to simplify the process of storing and accessing a specific type of data. These interfaces support

                                                                  the 8-bit raster image(DFR8), 24-bit raster image (DF 24), palette (DFP ), scientific data (DFSD ),

                                                                  and annotation (DFAN ) models. All single-file interfaces are built upon the H routines - unless

                                                                  otherwise specified, all the low-level details can be ignored.

                                                                  1.4.1 24-bit Raster Image Sets: DF24 Interface

                                                                  The HDF 24-bit raster interface provides a collection of routines for managing 24-bit raster image

                                                                  sets. A 24-bit raster image set is comprised of a 24-bit raster image array and its accompanied

                                                                  dimension record. Raster image sets may also include a palette.

                                                                  The names of the routines in the 24-bit raster interface are prefaced by ´DF 24´. The equivalent

                                                                  FORTRAN -77 routine names are prefaced by d́2´.

                                                                  1.4.2 8-bit Raster Image Sets: DFR8 Interface

                                                                  The HDF 8-bit raster interface provides a collection of routines for managing 8-bit raster image

                                                                  sets. An 8-bit raster image set is comprised of an 8-bit raster image array and its accompanied

                                                                  dimension record. Raster image sets may also include a palette.

                                                                  Every function in the 8-bit raster interface begins with the prefix ´DFR8´. The equivalent FO R-

                                                                  TRAN-77 functions use the prefix d́8´.

                                                                  1.4.3 Palettes: DFP Interface

                                                                  The HDF palette interface provides a collection of routines for managing palette data. This inter-

                                                                  face is most often used for working with multiple palettes stored in a single file or palettes not spe-

                                                                  cifically assigned to a raster image.

                                                                  The names of the routines in the palette interface are prefaced by ´DFP´. The equivalent FOR-

                                                                  TRAN-77 routine names are prefaced by d́p´.

                                                                  1.4.4 Scientific Data Sets: DFSD Interface

                                                                  There are two HDF interfaces that support multidimensional arrays: the single-file DF SD inter-

                                                                  face described here, which permits access to only one file at a time, and the newer multifile SD

                                                                  interface, which permits simultaneous access to more than one file.  The existence of the single-

                                                                  file scientific data set interface is simply to support backward compatibility for previously created

                                                                  files and applications.  It is recommended that the multifile scientific data set interface is to be

                                                                  used where possible.

                                                                  The single-file scientific data set interface provides a collection of routines for reading and writing

                                                                  arrays of data. A  scientific data set is comprised of a scientific data array and its accompanied

                                                                  rank, name and number type. Scientific data sets may also include predefined attribute records.

                                                                  June 25, 1998 1-5

                                                                  The names of the routines in the single-file scientific data set interface are prefaced by ´D FSD´.

                                                                  The equivalent FORTRAN-77 routine names are prefaced by d́s´.

                                                                  1.4.5 Annotations: DFAN Interface

                                                                  The single-file annotation interface provides a collection of routines for reading and writing text

                                                                  strings assigned to HDF data objects or files. Annotations consist of labels and descriptions.

                                                                  The names of the routines in the single-file annotation interface are prefaced by ´DFAN´. The

                                                                  equivalent FORTRAN-77 routine names are prefaced by d́a´.

                                             1.5 FORTRAN-77 and C Language Issues

                                                                  In order to make the FORTRAN-77 and C versions of each routine as similar as possible, some

                                                                  compromises have been made in the process of simplifying the interface for both programming

                                                                  languages.

                                                                  1.5.1 FORTRAN-77-to-C Translation

                                                                  Nearly all of the HDF library code is written in C. The Fortran HDF API routines translate all

                                                                  parameter data types to C data types, then call the C routine that performs the main function. For

                                                                  example, d8aimg  is the FORTRAN -77 equivalent for DFR 8add image . Calls to either routine

                                                                  execute the same C code that adds an 8-bit raster image to an HDF file - see the following figure.

FIGURE 2b

                                                                  Use of a Function Call Converter to Route FORTRA N-77 HDF Calls to th e C Lib rary

                                                                  1.5.2 Case Sensitivity

                                                                  FORTRAN -77 identifiers generally are not case sensitive, whereas C identifiers are. Although all

                                                                  of the FORTRAN-77 routines shown in this manual are written in lower case, FORTRA N-77 pro-

                                                                  grams can generally call them using either upper- or lower-case letters without loss of meaning.

                                                                  1.5.3 Name Length

                                                                  Because some F ORTRAN-77 compilers only interpret identifier names with seven or fewer char-

                                                                  acters, the first seven characters of the FORTRAN-77 HDF  routine names are unique.

                                                                  1.5.4 Header Files

                                                                  The inclusion of header files is not generally permitted by FORTRAN-77 compilers. However, it

                                                                  is sometimes available as an option. On UNIX systems, for example, the macro processors
m4

 and

                                                                                  Your
                                                                                     C
                                                                             Program

                                                                        DFR8addimage

Your
FORTRAN-77
Program

d8aimg

FORTRAN-77 to C

HDF Library
d8aimg to DFR8addimage

1-6 June 25, 1998

                                                                  cpp

                                                                               let the compiler include and preprocess header files. If this capability is not available, the user

                                                                  may have to copy the declarations, definitions, and values needed from the files
dffunc.inc

 and

                                                                  hdf.inc

                                                                                             into the user application. If the capability is available, the files can be included in the

                                                                  Fortran code.  The files reside in the
include/

 subdirectory of the directory where the HDF

                                                                  library is installed on the userś system.

                                                                  1.5.5 Data Type Specifications

                                                                  When mixing machines, compilers, and languages, it is difficult to maintain consistent data type

                                                                  definitions. For instance, on some machines an integer is a 32-bit quantity and on others, a 16-bit

                                                                  quantity. In addition, the differences between F ORTRAN-77 and C lead to difficulties in describ-

                                                                  ing the data types found in the argument lists of HDF  routines. To maintain portability, the HDF

                                                                  library expects assigned names for all data types used in HD F routines. (See TABLE 1A)

TABLE 1A

                                                                  Data Type Definitions

                                                                  When using a FORTRAN-77 data type that is not supported, the general practice is to use another

                                                                  data type of the same size. For example, an 8-bit signed integer can be used to store an 8-bit

                                                                  unsigned integer variable unless the code relies on a sign-specific operation.

                                                                                       Definition Name Definition Value Description

                                                                                        DFNT_CHAR8 4 8-bit character type

                                                                                         DFNT_CHAR 4 Same as DFNT_CHAR8

                                                                                      DFNT_UCHAR8 3 8-bit unsigned character type

                                                                                        DFNT_UCHAR 3 Same as DFNT_UCHAR8

                                                                                           DFNT_INT8 20 8-bit integer type

                                                                                         DFNT_UINT8 21 8-bit unsigned integer type

                                                                                          DFNT_INT16 22 16-bit integer type

                                                                                        DFNT_UINT16 23 16-bit unsigned integer type

                                                                                          DFNT_INT32 24 32-bit integer type

                                                                                        DFNT_UINT32 25 32-bit unsigned integer type

                                                                                          DFNT_INT64 26 64-bit integer type

                                                                                        DFNT_UINT64 27 64-bit unsigned integer type

                                                                                      DFNT_FLOAT32 5 32-bit floating-point type

                                                                                      DFNT_FLOAT64 6 64-bit floating-point type

                                                                                         DFNT_NINT8 (DFNT_NATIVE | DFNT_INT8 8-bit native integer type

                                                                                        DFNT_NUINT8 (DFNT_NATIVE | DFNT_UINT8) 8-bit native unsigned integer type

                                                                                        DFNT_NINT16 (DFNT_NATIVE | DFNT_INT16) 16-bit native integer type

                                                                                      DFNT_NUINT16 (DFNT_NATIVE | DFNT_UINT16) 16-bit native unsigned integer type

                                                                                        DFNT_NINT32 (DFNT_NATIVE | DFNT_INT32) 32-bit native integer type

                                                                                      DFNT_NUINT32 (DFNT_NATIVE | DFNT_UINT32) 32-bit native unsigned integer type

                                                                                        DFNT_NINT64 (DFNT_NATIVE | DFNT_INT64) 64-bit native integer type

                                                                                      DFNT_NUINT64 (DFNT_NATIVE | DFNT_UINT64) 64-bit native unsigned integer type

                                                                                    DFNT_NFLOAT32 (DFNT_NATIVE | DFNT_FLOAT32) 32-bit native floating-point type

                                                                                    DFNT_NFLOAT64 (DFNT_NATIVE | DFNT_FLOAT64) 64-bit native floating-point type

                                                                  June 25, 1998 1-7

                                                                  1.5.6 String and Array Specifications

                                                                  In the declarations contained in the headers of FORTRAN-77 functions, the following conven-

                                                                  tions are followed:

                                                                           ¯ character*(*) x

 means that
 x
refers to a string of an indefinite number of characters. It

                                                                                  is the responsibility of the calling program to allocate enough space to hold the data to be

                                                                                  stored in the string.

                                                                           ¯ real x(*)

                                                                                                                     means that
 x
refers to an array of reals of indefinite size and of indefinite rank.

                                                                                  It is the responsibility of the calling program to allocate an actual array with the correct

                                                                                  number of dimensions and dimension sizes.

                                                                           ¯ <valid numeric data type >
x
means that
 x
may have one of the numeric data types

                                                                                  listed in the Description column of Table 1A .

                                                                           ¯ <valid data type >
x
means that
 x
may have any of the data types listed in the Descrip-

                                                                                  tion column of Table 1A.

                                                                  1.5.7 FORTRAN-77, ANSI C and K&R C

                                                                  As much as possible, we have conformed the HDF API routines to those implementations of For-

                                                                  tran and C that are in most common use today, namely FORTRAN-77, ANSI C and K&R C. Due

                                                                  to the increasing availability of ANSI C, future versions of HDF will no longer support K&R C.

                                                                  As Fortran-90 is a superset of FORTRAN-77, H DF programs should compile and run correctly

                                                                  when using a Fortran-90 compiler.

                                             1.6 Error Codes

                                                                  The error codes defined in the HDF  library are listed in the following table.

TABLE 1B

                                                                  HDF Error Codes

                                                                                       Error Code Code Definition

                                                                                      DFE_NONE No error.

                                                                                        DFE_FNF File not found.

                                                                                    DFE_DENIED Access to file denied.

                                                                                  DFE_ALROPEN File already open.

                                                                                DFE_TOOMANY Too many AID’s or files open.

                                                                                 DFE_BADNAME Bad file name on open.

                                                                                   DFE_BADACC Bad file access mode.

                                                                                  DFE_BADOPEN Miscellaneous  open error.

                                                                                  DFE_NOTOPEN File can’t be closed because it hasn´t been opened.

                                                                               DFE_CANTCLOSE fclose  error

                                                                              DFE_READERROR Read error.

                                                                             DFE_WRITEERROR Write error.

                                                                               DFE_SEEKERROR Seek error.

                                                                                   DFE_RDONLY File is read only.

                                                                                  DFE_BADSEEK Attempt to seek past end of element.

                                                                                  DFE_PUTELEM Hputelement  error.

                                                                                  DFE_GETELEM Hgetelement  error.

1-8 June 25, 1998

                                                                                 DFE_CANTLINK Cannot initialize link information.

                                                                                DFE_CANTSYNC Cannot synchronize memory with file.

                                                                                DFE_BADGROUP Error from DFdiread  in opening a group.

                                                                             DFE_GROUPSETUP Error from DFdisetup  in opening a group.

                                                                                DFE_PUTGROUP Error on  putting a tag/reference number pair into a group.

                                                                             DFE_GROUPWRITE Error when writing group contents.

                                                                                   DFE_DFNULL Data file reference is a null pointer.

                                                                                   DFE_ILLTYPE Data file contains an illegal type: internal error.

                                                                               DFE_BADDDLIST The DD list is non-existent: internal error.

                                                                                DFE_NOTDFFILE The current file is not an HDF file and it is not zero length.

                                                                               DFE_SEEDTWICE The DD list already seeded: internal error.

                                                                              DFE_NOSUCHTAG No such tag in the file: search failed.

                                                                                DFE_NOFREEDD There are no free DD’s left: internal error.

                                                                                   DFE_BADTAG Illegal WILDCARD tag.

                                                                                    DFE_BADREF Illegal WILDCARD reference number.

                                                                                 DFE_NOMATCH No DDs (or no more DDs) that match the specified tag/reference number pair.

                                                                                 DFE_NOTINSET Warning: Set contained unknown tag. Ignored.

                                                                               DFE_BADOFFSET Illegal offset specified.

                                                                                  DFE_CORRUPT File is corrupted.

                                                                                     DFE_NOREF No more reference numbers are available.

                                                                                     DFE_DUPDD The new tag/reference number pair has been allocated.

                                                                                 DFE_CANTMOD Old element doesn´t exist.  Cannot modify.

                                                                                 DFE_DIFFFILES Attempt to merge objects in different files.

                                                                                    DFE_BADAID An invalid AID was received.

                                                                                  DFE_OPENAID Active AIDs still exist.

                                                                               DFE_CANTFLUSH Cannot flush DD back to file.

                                                                             DFE_CANTUPDATE Cannot update the DD block.

                                                                                DFE_CANTHASH Cannot add a DD to the hash table.

                                                                              DFE_CANTDELDD Cannot delete a DD in the file.

                                                                           DFE_CANTDELHASH Cannot delete a DD from the hash table.

                                                                              DFE_CANTACCESS Cannot access specified tag/reference number pair.

                                                                        DFE_CANTENDACCESS Cannot end access to data element.

                                                                               DFE_TABLEFULL Access table is full.

                                                                              DFE_NOTINTABLE Cannot find element in table.

                                                                            DFE_UNSUPPORTED Feature not currently supported.

                                                                                  DFE_NOSPACE malloc  failed.

                                                                                  DFE_BADCALL Routine calls were in the wrong order.

                                                                                    DFE_BADPTR NULL pointer argument was specified.

                                                                                   DFE_BADLEN Invalid length was specified.

                                                                              DFE_NOTENOUGH Not enough space for the data.

                                                                                    DFE_NOVALS Values were not available.

                                                                                      DFE_ARGS Invalid arguments passed to the routine.

                                                                                 DFE_INTERNAL Serious internal error.

                                                                                  DFE_NORESET Too late to modify this value.

                                                                                    DFE_GENAPP Generic application level error.

                                                                                     DFE_UNINIT Interface was not initialized correctly.

                                                                                  DFE_CANTINIT Cannot initialize the interface the operation requires.

                                                                                       Error Code Code Definition

June 25, 1998 1-9

      DFE_CANTSHUTDOWN Cannot shut down the interface the operation requires.

                 DFE_BADDIM Negative number of dimensions, or zero dimensions, was specified.

                   DFE_BADFP File contained an illegal floating point number.

          DFE_BADDATATYPE Unknown or unavailable data type was specified.

            DFE_BADMCTYPE Unknown or unavailable machine type was specified.

          DFE_BADNUMTYPE Unknown or unavailable number type was specified.

             DFE_BADORDER Unknown or illegal array order was specified.

                  DFE_RANGE Improper range for attempted access.

               DFE_BADCONV Invalid data type conversion was specified.

                DFE_BADTYPE Incompatible types were specified.

            DFE_BADSCHEME Unknown compression scheme was specified.

             DFE_BADMODEL Invalid compression model was specified.

             DFE_BADCODER Invalid compression encoder was specified.

                  DFE_MODEL Error in the modeling layer of the compression operation.

                  DFE_CODER Error in the encoding layer of the compression operation.

                    DFE_CINIT Error in encoding initialization.

               DFE_CDECODE Error in decoding compressed data.

               DFE_CENCODE Error in encoding compressed data.

                  DFE_CTERM Error in encoding termination.

                   DFE_CSEEK Error seeking in an encoded dataset.

                    DFE_MINIT Error in modeling initialization.

              DFE_COMPINFO Invalid compression header.

             DFE_CANTCOMP Cannot compress an object.

          DFE_CANTDECOMP Cannot decompress an object.

                  DFE_NODIM A dimension record was not associated with the image.

                 DFE_BADRIG Error processing a RIG.

           DFE_RINOTFOUND Cannot find raster image.

                DFE_BADATTR Invalid attribute.

              DFE_BADTABLE The nsdg table has incorrect information.

                 DFE_BADSDG Error in processing an SDG.

                DFE_BADNDG Error in processing an NDG.

                  DFE_VGSIZE Too many elements in the vgroup.

                    DFE_VTAB Element not in vtab[].

         DFE_CANTADDELEM Cannot add the  tag/reference number pair to the vgroup.

           DFE_BADVGNAME Cannot set the vgroup name.

           DFE_BADVGCLASS Cannot set the vgroup class.

             DFE_BADFIELDS Invalid fields string passed to vset routine.

                    DFE_NOVS Cannot find the vset in the file.

                DFE_SYMSIZE Too many symbols in the users table.

             DFE_BADATTACH Cannot write to a previously attached vdata.

            DFE_BADVSNAME Cannot set the vdata name.

           DFE_BADVSCLASS Cannot set the vdata class.

                DFE_VSWRITE Error writing to the vdata.

                 DFE_VSREAD Error reading from the vdata.

                  DFE_BADVH Error in the vdata header.

        DFE_VSCANTCREATE Cannot create the vdata.

        DFE_VGCANTCREATE Cannot create the vgroup.

                     Error Code Code Definition

1-10 June 25, 1998

                                                                             DFE_CANTATTACH Cannot attach to a vdata or vset.

                                                                             DFE_CANTDETACH Cannot detach a vdata or vset with write access.

                                                                                  DFE_BITREAD A bit read error occurred.

                                                                                 DFE_BITWRITE A bit write error occurred.

                                                                                   DFE_BITSEEK A bit seek error occurred.

                                                                                   DFE_TBBTINS Failed to insert the element into tree.

                                                                                    DFE_BVNEW Failed to create a bit vector.

                                                                                     DFE_BVSET Failed when setting a bit in a bit vector.

                                                                                     DFE_BVGET Failed when getting a bit in a bit vector.

                                                                                    DFE_BVFIND Failed when finding a bit in a bit vector.

                                                                                       Error Code Code Definition